__S0 800 0 ABS
__S1 78 0 ABS
__Hintentry 0 0 CODE
__Lintentry 0 0 CODE
_FPB0 30 0 ABS
_main 7AB 0 CODE
btemp 7E 0 ABS
_exit 0 0 CODE
start 0 0 CODE
_TRISA 85 0 ABS
_TRISB 86 0 ABS
_PORTA 5 0 ABS
reset_vec 0 0 CODE
_PORTB 6 0 ABS
_EEADR 10D 0 ABS
_EECON 110 0 ABS
wtemp0 7E 0 ABS
delay_ms@m 72 0 COMMON
__Hconfig 0 0 CONFIG
__Lconfig 0 0 CONFIG
delay_ms@n 74 0 COMMON
__Hram 0 0 ABS
__Lram 0 0 ABS
?_main 70 0 COMMON
EEPROM_Read_1Byte@EEPROM_Addr 70 0 COMMON
__size_of_EEPROM_Read_1Byte 0 0 ABS
__Hfunctab 0 0 CODE
__Lfunctab 0 0 CODE
_OPTION_REG 81 0 ABS
__Hcommon 0 0 ABS
__Lcommon 0 0 ABS
__Heeprom_data 0 0 EEDATA
__Leeprom_data 0 0 EEDATA
_delay_ms 7E0 0 CODE
_EEDATL 10E 0 ABS
__Habs1 0 0 ABS
__Labs1 0 0 ABS
__Hsfr0 0 0 ABS
__Lsfr0 0 0 ABS
__Hsfr1 0 0 ABS
__Lsfr1 0 0 ABS
__Hsfr2 0 0 ABS
__Lsfr2 0 0 ABS
__Hsfr3 0 0 ABS
__Lsfr3 0 0 ABS
delay_ms@x 70 0 COMMON
__Hcode 0 0 ABS
__Lcode 0 0 ABS
??_main 78 0 COMMON
??_GPIO_Init 70 0 COMMON
__Hinit 0 0 CODE
__Linit 0 0 CODE
__end_of_main 7C2 0 CODE
__Htext 0 0 ABS
__Ltext 0 0 ABS
end_of_initialization 78F 0 CODE
_GPIO_Init 791 0 CODE
EEPROM_Write_1Byte@EEPROM_Addr 77 0 COMMON
_FREADEE 880 0 ABS
?_EEPROM_Read_1Byte 70 0 COMMON
?_delay_ms 70 0 COMMON
__Hstrings 0 0 ABS
__Lstrings 0 0 ABS
_FTIMEEE 886 0 ABS
_FPROGEE 881 0 ABS
__Hbank0 0 0 ABS
__Lbank0 0 0 ABS
__Hbank1 0 0 ABS
__Lbank1 0 0 ABS
__Hbank2 0 0 BANK2
__Lbank2 0 0 BANK2
__Hbank3 0 0 BANK3
__Lbank3 0 0 BANK3
__Hpowerup 0 0 CODE
__Lpowerup 0 0 CODE
__end_of_EEPROM_Read_1Byte 7AB 0 CODE
__Hclrtext 0 0 ABS
__Lclrtext 0 0 ABS
__Hidloc 0 0 IDLOC
__Lidloc 0 0 IDLOC
__size_of_delay_ms 0 0 ABS
__Hcinit 0 0 ABS
__Lcinit 0 0 ABS
?_EEPROM_Write_1Byte 76 0 COMMON
__size_of_main 0 0 ABS
__size_of_EEPROM_Write_1Byte 0 0 ABS
__end_of_GPIO_Init 79D 0 CODE
?_GPIO_Init 70 0 COMMON
__end_of_EEPROM_Write_1Byte 7E0 0 CODE
EEPROM_Read_1Byte@ReadEeprom_Data 71 0 COMMON
_EEPROM_Write_1Byte 7C2 0 CODE
__ptext64 0 0 CODE
__ptext65 7C2 0 CODE
EEPROM_Write_1Byte@EEPROM_Data 76 0 COMMON
__ptext66 79D 0 CODE
??_delay_ms 72 0 COMMON
__ptext67 7E0 0 CODE
_FERASEEE 882 0 ABS
__ptext68 791 0 CODE
__ptext69 0 0 CODE
__Hend_init 1 0 CODE
__Lend_init 0 0 CODE
__end_of_delay_ms 800 0 CODE
??_EEPROM_Write_1Byte 77 0 COMMON
__Hreset_vec 0 0 CODE
__Lreset_vec 0 0 CODE
intlevel0 0 0 CODE
intlevel1 0 0 CODE
intlevel2 0 0 CODE
intlevel3 0 0 CODE
intlevel4 0 0 CODE
intlevel5 0 0 CODE
__HcstackCOMMON 0 0 ABS
__LcstackCOMMON 0 0 ABS
__size_of_GPIO_Init 0 0 ABS
__pcstackCOMMON 70 0 COMMON
start_initialization 78F 0 CODE
__Hmaintext 0 0 ABS
__Lmaintext 0 0 ABS
__pmaintext 7AB 0 CODE
??_EEPROM_Read_1Byte 70 0 COMMON
_EEPROM_Read_1Byte 79D 0 CODE
%segments
reset_vec 0 1 CODE 0
cstackCOMMON 70 77 COMMON 70
text67 FC0 FFF CODE FC0
text65 F84 FBF CODE F84
maintext F56 F83 CODE F56
text66 F3A F55 CODE F3A
text68 F22 F39 CODE F22
cinit F1E F21 CODE F1E
%locals
startup.obj
startup.as
70 0 0 CODE
HS16F3211_EEPROM.obj
HS16F3211_EEPROM.as
89 78F 0 CODE
90 790 0 CODE
E:\PROJECT\应用方案\@应用相关文档整理\HS16F3211应用示范例程\HS16F3211_EEPROM\HS16F3211_EEPROM.c
118 7AB 0 CODE
119 7AC 0 CODE
120 7AD 0 CODE
123 7B1 0 CODE
124 7B2 0 CODE
126 7B9 0 CODE
128 7BC 0 CODE
130 7C2 0 CODE
66 7C2 0 CODE
67 7C3 0 CODE
77 7C6 0 CODE
78 7C7 0 CODE
79 7C9 0 CODE
80 7CA 0 CODE
81 7CD 0 CODE
82 7CE 0 CODE
83 7D4 0 CODE
84 7D6 0 CODE
85 7D7 0 CODE
86 7DB 0 CODE
88 7DF 0 CODE
99 79D 0 CODE
108 7A1 0 CODE
109 7A3 0 CODE
110 7A4 0 CODE
111 7A5 0 CODE
112 7A9 0 CODE
113 7AA 0 CODE
52 7E0 0 CODE
54 7E3 0 CODE
55 7E5 0 CODE
54 7E6 0 CODE
52 7F2 0 CODE
57 7FF 0 CODE
29 791 0 CODE
36 794 0 CODE
37 796 0 CODE
39 798 0 CODE
40 79A 0 CODE
42 79C 0 CODE
