;=======================================================================
; Installation inf for the SONIX S9KD USB MULTIMEDIA DEVICE
;
; (c) Copyright 2011 
;
; Last modified: 2011-08-05
;
; Number of PID: 128
;
; Only supply Windows Win7/XP/2K OS
;=======================================================================

[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%MFG%
CatalogFile.NT = SN8USB2PRT.cat
DriverVer=08/05/2011, 1.3.0.1

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]                ; Update driver for Window 7
%MfgName%=SNX, NTamd64, NTia64

[SNX]
%USB\VID_0c45&PID_5000.DeviceDesc%=USB2PRT, USB\VID_0c45&PID_5000

[SNX.NTamd64]
%USB\VID_0c45&PID_5000.DeviceDesc%=USB2PRT.amd64, USB\VID_0c45&PID_5000

[SNX.NTia64]
%USB\VID_0c45&PID_5000.DeviceDesc%=USB2PRT.ia64, USB\VID_0c45&PID_5000

[PreCopySection]
HKR,,NoSetupUI,,1

[SourceDisksNames]
1='',,,

[SourceDisksFiles] ; files for Windows 98/ME
SN8USB2PRT98.SYS = 1

[SourceDisksFiles.x86] ; files for Windows 2000/XP/Vista/Win7 32 bits
SN8USB2PRTXP.SYS = 1

[SourceDisksFiles.amd64] ; files for Windows XP/Vista/Win7 64 bits
SN8USB2PRT64.sys = 1

[SourceDisksFiles.ia64] ; files for 64-bit Windows XP/Vista/7
SN8USB2PRTIA64.sys = 1

[DestinationDirs]
DefaultDestDir = 12
USB2PRT98.CopyList = 10, system32\drivers
USB2PRTXP.CopyList = 10, system32\drivers
USB2PRTamd64.CopyList = 10, system32\drivers
USB2PRTia64.CopyList = 10, system32\drivers

[USB2PRT]
DriverVer = 07/18/2003, 1.0.1.0
CopyFiles = USB2PRT98.CopyList
AddReg    = USB2PRT98.AddReg

[USB2PRT.NT]
DriverVer = 08/05/2011, 1.3.0.1
CopyFiles = USB2PRTXP.CopyList
AddReg    = USB2PRTXP.AddReg

[USB2PRT.amd64]
DriverVer = 08/05/2011, 1.3.0.1
CopyFiles = USB2PRTamd64.CopyList
AddReg    = USB2PRTamd64.AddReg

[USB2PRT.ia64]
DriverVer = 08/05/2011, 1.3.0.1
CopyFiles = USB2PRTia64.CopyList
AddReg    = USB2PRTia64.AddReg

[USB2PRT98.CopyList]
SN8USB2PRT98.SYS

[USB2PRTXP.CopyList]
SN8USB2PRTXP.SYS

[USB2PRTamd64.CopyList]
SN8USB2PRT64.sys

[USB2PRTia64.CopyList]
SN8USB2PRTIA64.sys

[USB2PRT.Services]
Addservice = SN8USB2PRT98, 0x00000002, USB2PRT98.AddService

[USB2PRT.NT.Services]
Addservice = SN8USB2PRTXP, 0x00000002, USB2PRTXP.AddService

[USB2PRT.amd64.Services]
Addservice = SN8USB2PRT64, 0x00000002, USB2PRTamd64.AddService

[USB2PRT.ia64.Services]
Addservice = SN8USB2PRTIA64, 0x00000002, USB2PRTia64.AddService

[USB2PRT98.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SN8USB2PRT98.SYS
HKR,,DriverFlags,0x00010001,0x00000001
HKLM,"System\Currentcontrolset\Services\SN8USB2PRT98","DebugLevel",0x10001,3
HKLM,"System\Currentcontrolset\services\SN8USB2PRT98","SSEnable",0x10001,0

[USB2PRTXP.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SN8USB2PRTXP.SYS
HKR,,DriverFlags,0x00010001,0x00000001
HKLM,"System\Currentcontrolset\Services\SN8USB2PRTXP","DebugLevel",0x10001,3
HKLM,"System\Currentcontrolset\services\SN8USB2PRTXP","SSEnable",0x10001,0

[USB2PRTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SN8USB2PRT64.SYS
HKR,,DriverFlags,0x00010001,0x00000001
HKLM,"System\Currentcontrolset\Services\SN8USB2PRT64","DebugLevel",0x10001,3
HKLM,"System\Currentcontrolset\services\SN8USB2PRT64","SSEnable",0x10001,0

[USB2PRTia64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SN8USB2PRTIA64.SYS
HKR,,DriverFlags,0x00010001,0x00000001
HKLM,"System\Currentcontrolset\Services\SN8USB2PRTIA64","DebugLevel",0x10001,3
HKLM,"System\Currentcontrolset\services\SN8USB2PRTIA64","SSEnable",0x10001,0

[USB2PRT98.AddService]
DisplayName    = %USB2PRT.SvcDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\SN8USB2PRT98.SYS
;LoadOrderGroup = USB

[USB2PRTXP.AddService]
DisplayName    = %USB2PRT.SvcDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\SN8USB2PRTXP.SYS
;LoadOrderGroup = USB

[USB2PRTamd64.AddService]
DisplayName    = %USB2PRT.SvcDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\SN8USB2PRT64.SYS
;LoadOrderGroup = USB

[USB2PRTia64.AddService]
DisplayName    = %USB2PRT.SvcDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\SN8USB2PRTIA64.SYS
;LoadOrderGroup = USB

[Strings]              
MFG="Sonix" 
MfgName="Sonix"
USB\VID_0c45&PID_5000.DeviceDesc="SONiX SN8 USB to Printer Port ICE/Writer"
USB2PRT.SvcDesc="SONiX SN8 USB to Printer Port ICE/Writer"

