opt subtitle "HI-TECH Software Omniscient Code Generator (PRO mode) build 10920"

opt pagewidth 120

	opt pm

	processor	16F685
clrc	macro
	bcf	3,0
	endm
clrz	macro
	bcf	3,2
	endm
setc	macro
	bsf	3,0
	endm
setz	macro
	bsf	3,2
	endm
skipc	macro
	btfss	3,0
	endm
skipz	macro
	btfss	3,2
	endm
skipnc	macro
	btfsc	3,0
	endm
skipnz	macro
	btfsc	3,2
	endm
indf	equ	0
indf0	equ	0
pc	equ	2
pcl	equ	2
status	equ	3
fsr	equ	4
fsr0	equ	4
c	equ	1
z	equ	0
pclath	equ	10
	FNCALL	_main,_GPIO_Init
	FNCALL	_main,_CLR_BANK0_RAM
	FNCALL	_main,_CLR_BANK1_RAM
	FNCALL	_main,_WDT_Init
	FNCALL	_main,_DelayUs
	FNROOT	_main
	FNCALL	intlevel1,_myIsr
	global	intlevel1
	FNROOT	intlevel1
	global	_temp
psect	nvCOMMON,class=COMMON,space=1
global __pnvCOMMON
__pnvCOMMON:
_temp:
       ds      1

	global	_FSR
_FSR	set	4
	global	_INDF
_INDF	set	0
	global	_ODCON
_ODCON	set	15
	global	_PDCON
_PDCON	set	14
	global	_PHCON
_PHCON	set	16
	global	_PORTA
_PORTA	set	5
	global	_PORTB
_PORTB	set	6
	global	_FT0IF
_FT0IF	set	96
	global	_OPTION_REG
_OPTION_REG	set	129
	global	_PADCON
_PADCON	set	147
	global	_PAHCON
_PAHCON	set	146
	global	_PAIC0
_PAIC0	set	144
	global	_PBIC0
_PBIC0	set	145
	global	_PCON
_PCON	set	142
	global	_PDCON2
_PDCON2	set	147
	global	_TRISA
_TRISA	set	133
	global	_TRISB
_TRISB	set	134
	global	_WUCON
_WUCON	set	143
	file	"HS16F1211_wdt.as"
	line	#
psect cinit,class=CODE,delta=2
global start_initialization
start_initialization:

psect cinit,class=CODE,delta=2
global end_of_initialization

;End of C runtime variable initialization code

end_of_initialization:
clrf status
ljmp _main	;jump to C main() function
psect	cstackCOMMON,class=COMMON,space=1
global __pcstackCOMMON
__pcstackCOMMON:
	global	?_GPIO_Init
?_GPIO_Init:	; 0 bytes @ 0x0
	global	?_CLR_BANK0_RAM
?_CLR_BANK0_RAM:	; 0 bytes @ 0x0
	global	?_CLR_BANK1_RAM
?_CLR_BANK1_RAM:	; 0 bytes @ 0x0
	global	?_WDT_Init
?_WDT_Init:	; 0 bytes @ 0x0
	global	?_DelayUs
?_DelayUs:	; 0 bytes @ 0x0
	global	?_myIsr
?_myIsr:	; 0 bytes @ 0x0
	global	??_myIsr
??_myIsr:	; 0 bytes @ 0x0
	global	?_main
?_main:	; 0 bytes @ 0x0
	ds	2
	global	??_GPIO_Init
??_GPIO_Init:	; 0 bytes @ 0x2
	global	??_CLR_BANK0_RAM
??_CLR_BANK0_RAM:	; 0 bytes @ 0x2
	global	??_CLR_BANK1_RAM
??_CLR_BANK1_RAM:	; 0 bytes @ 0x2
	global	??_WDT_Init
??_WDT_Init:	; 0 bytes @ 0x2
	global	??_DelayUs
??_DelayUs:	; 0 bytes @ 0x2
	global	DelayUs@delayUs
DelayUs@delayUs:	; 1 bytes @ 0x2
	ds	1
	global	??_main
??_main:	; 0 bytes @ 0x3
;;Data sizes: Strings 0, constant 0, data 0, bss 0, persistent 1 stack 0
;;Auto spaces:   Size  Autos    Used
;; COMMON          14      3       4
;; BANK0           48      0       0

;;
;; Pointer list with targets:



;;
;; Critical Paths under _main in COMMON
;;
;;   _main->_DelayUs
;;
;; Critical Paths under _myIsr in COMMON
;;
;;   None.
;;
;; Critical Paths under _main in BANK0
;;
;;   None.
;;
;; Critical Paths under _myIsr in BANK0
;;
;;   None.

;;
;;Main: autosize = 0, tempsize = 0, incstack = 0, save=0
;;

;;
;;Call Graph Tables:
;;
;; ---------------------------------------------------------------------------------
;; (Depth) Function   	        Calls       Base Space   Used Autos Params    Refs
;; ---------------------------------------------------------------------------------
;; (0) _main                                                 0     0      0      15
;;                          _GPIO_Init
;;                      _CLR_BANK0_RAM
;;                      _CLR_BANK1_RAM
;;                           _WDT_Init
;;                            _DelayUs
;; ---------------------------------------------------------------------------------
;; (1) _DelayUs                                              1     1      0      15
;;                                              2 COMMON     1     1      0
;; ---------------------------------------------------------------------------------
;; (1) _WDT_Init                                             0     0      0       0
;; ---------------------------------------------------------------------------------
;; (1) _CLR_BANK1_RAM                                        0     0      0       0
;; ---------------------------------------------------------------------------------
;; (1) _CLR_BANK0_RAM                                        0     0      0       0
;; ---------------------------------------------------------------------------------
;; (1) _GPIO_Init                                            0     0      0       0
;; ---------------------------------------------------------------------------------
;; Estimated maximum stack depth 1
;; ---------------------------------------------------------------------------------
;; (Depth) Function   	        Calls       Base Space   Used Autos Params    Refs
;; ---------------------------------------------------------------------------------
;; (2) _myIsr                                                2     2      0       0
;;                                              0 COMMON     2     2      0
;; ---------------------------------------------------------------------------------
;; Estimated maximum stack depth 2
;; ---------------------------------------------------------------------------------

;; Call Graph Graphs:

;; _main (ROOT)
;;   _GPIO_Init
;;   _CLR_BANK0_RAM
;;   _CLR_BANK1_RAM
;;   _WDT_Init
;;   _DelayUs
;;
;; _myIsr (ROOT)
;;

;; Address spaces:

;;Name               Size   Autos  Total    Cost      Usage
;;BITCOMMON            E      0       0       0        0.0%
;;NULL                 0      0       0       0        0.0%
;;CODE                 0      0       0       0        0.0%
;;COMMON               E      3       4       1       28.6%
;;BITSFR0              0      0       0       1        0.0%
;;SFR0                 0      0       0       1        0.0%
;;BITSFR1              0      0       0       2        0.0%
;;SFR1                 0      0       0       2        0.0%
;;STACK                0      0       1       2        0.0%
;;ABS                  0      0       4       3        0.0%
;;BITSFR3              0      0       0       4        0.0%
;;SFR3                 0      0       0       4        0.0%
;;DATA                 0      0       5       4        0.0%
;;BITBANK0            30      0       0       5        0.0%
;;BITSFR2              0      0       0       5        0.0%
;;SFR2                 0      0       0       5        0.0%
;;BANK0               30      0       0       6        0.0%

	global	_main
psect	maintext,global,class=CODE,delta=2
global __pmaintext
__pmaintext:

;; *************** function _main *****************
;; Defined at:
;;		line 30 in file "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
;; Parameters:    Size  Location     Type
;;		None
;; Auto vars:     Size  Location     Type
;;		None
;; Return value:  Size  Location     Type
;;		None               void
;; Registers used:
;;		wreg, status,2, status,0, pclath, cstack
;; Tracked objects:
;;		On entry : 17F/0
;;		On exit  : 60/0
;;		Unchanged: FFE00/0
;; Data sizes:     COMMON   BANK0
;;      Params:         0       0
;;      Locals:         0       0
;;      Temps:          0       0
;;      Totals:         0       0
;;Total ram usage:        0 bytes
;; Hardware stack levels required when called:    2
;; This function calls:
;;		_GPIO_Init
;;		_CLR_BANK0_RAM
;;		_CLR_BANK1_RAM
;;		_WDT_Init
;;		_DelayUs
;; This function is called by:
;;		Startup code after reset
;; This function uses a non-reentrant model
;;
psect	maintext
	file	"E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
	line	30
	global	__size_of_main
	__size_of_main	equ	__end_of_main-_main
	
_main:	
	opt	stack 6
; Regs used in _main: [wreg+status,2+status,0+pclath+cstack]
	line	31
	
l1280:	
;main.c: 31: GPIO_Init();
	fcall	_GPIO_Init
	line	32
	
l1282:	
;main.c: 32: CLR_BANK0_RAM();
	fcall	_CLR_BANK0_RAM
	line	33
	
l1284:	
;main.c: 33: CLR_BANK1_RAM();
	fcall	_CLR_BANK1_RAM
	line	34
;main.c: 34: WDT_Init();
	fcall	_WDT_Init
	line	36
	
l1286:	
;main.c: 36: temp = 200;
	movlw	(0C8h)
	movwf	(_temp)
	line	37
;main.c: 37: while(temp--)
	goto	l845
	line	39
	
l1288:	
;main.c: 38: {
;main.c: 39: PORTA = PORTA^0x0f;
	movlw	(0Fh)
	bcf	status, 5	;RP0=0, select bank0
	bcf	status, 6	;RP1=0, select bank0
	xorwf	(5),f	;volatile
	line	40
	
l1290:	
# 40 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
clrwdt ;#
psect	maintext
	line	41
	
l845:	
	line	37
	decf	(_temp),f
	movf	((_temp)),w
	xorlw	0FFh
	skipz
	goto	u31
	goto	u30
u31:
	goto	l1288
u30:
	line	47
	
l1292:	
;main.c: 43: {
;main.c: 47: PORTA = PORTA^0xf0;
	movlw	(0F0h)
	bcf	status, 5	;RP0=0, select bank0
	bcf	status, 6	;RP1=0, select bank0
	xorwf	(5),f	;volatile
	line	49
	
l1294:	
;main.c: 49: DelayUs(1);
	movlw	(01h)
	fcall	_DelayUs
	goto	l1292
	global	start
	ljmp	start
	opt stack 0
psect	maintext
	line	51
GLOBAL	__end_of_main
	__end_of_main:
;; =============== function _main ends ============

	signat	_main,88
	global	_DelayUs
psect	text78,local,class=CODE,delta=2
global __ptext78
__ptext78:

;; *************** function _DelayUs *****************
;; Defined at:
;;		line 169 in file "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
;; Parameters:    Size  Location     Type
;;  delayUs         1    wreg     unsigned char 
;; Auto vars:     Size  Location     Type
;;  delayUs         1    2[COMMON] unsigned char 
;; Return value:  Size  Location     Type
;;		None               void
;; Registers used:
;;		wreg, status,2, status,0
;; Tracked objects:
;;		On entry : 60/0
;;		On exit  : 60/0
;;		Unchanged: FFF9F/0
;; Data sizes:     COMMON   BANK0
;;      Params:         0       0
;;      Locals:         1       0
;;      Temps:          0       0
;;      Totals:         1       0
;;Total ram usage:        1 bytes
;; Hardware stack levels used:    1
;; Hardware stack levels required when called:    1
;; This function calls:
;;		Nothing
;; This function is called by:
;;		_main
;; This function uses a non-reentrant model
;;
psect	text78
	file	"E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
	line	169
	global	__size_of_DelayUs
	__size_of_DelayUs	equ	__end_of_DelayUs-_DelayUs
	
_DelayUs:	
	opt	stack 6
; Regs used in _DelayUs: [wreg+status,2+status,0]
;DelayUs@delayUs stored from wreg
	movwf	(DelayUs@delayUs)
	line	170
	
l1276:	
;main.c: 170: while(delayUs--);
	
l1278:	
	decf	(DelayUs@delayUs),f
	movf	((DelayUs@delayUs)),w
	xorlw	0FFh
	skipz
	goto	u21
	goto	u20
u21:
	goto	l1278
u20:
	line	171
	
l869:	
	return
	opt stack 0
GLOBAL	__end_of_DelayUs
	__end_of_DelayUs:
;; =============== function _DelayUs ends ============

	signat	_DelayUs,4216
	global	_WDT_Init
psect	text79,local,class=CODE,delta=2
global __ptext79
__ptext79:

;; *************** function _WDT_Init *****************
;; Defined at:
;;		line 69 in file "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
;; Parameters:    Size  Location     Type
;;		None
;; Auto vars:     Size  Location     Type
;;		None
;; Return value:  Size  Location     Type
;;		None               void
;; Registers used:
;;		wreg
;; Tracked objects:
;;		On entry : 0/0
;;		On exit  : 60/20
;;		Unchanged: FFE00/0
;; Data sizes:     COMMON   BANK0
;;      Params:         0       0
;;      Locals:         0       0
;;      Temps:          0       0
;;      Totals:         0       0
;;Total ram usage:        0 bytes
;; Hardware stack levels used:    1
;; Hardware stack levels required when called:    1
;; This function calls:
;;		Nothing
;; This function is called by:
;;		_main
;; This function uses a non-reentrant model
;;
psect	text79
	file	"E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
	line	69
	global	__size_of_WDT_Init
	__size_of_WDT_Init	equ	__end_of_WDT_Init-_WDT_Init
	
_WDT_Init:	
	opt	stack 6
; Regs used in _WDT_Init: [wreg]
	line	70
	
l1272:	
# 70 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
clrwdt ;#
psect	text79
	line	73
	
l1274:	
;main.c: 73: OPTION_REG= 0b00001000;
	movlw	(08h)
	bsf	status, 5	;RP0=1, select bank1
	bcf	status, 6	;RP1=0, select bank1
	movwf	(129)^080h	;volatile
	line	82
;main.c: 82: PCON = 0b10000000;
	movlw	(080h)
	movwf	(142)^080h	;volatile
	line	86
	
l854:	
	return
	opt stack 0
GLOBAL	__end_of_WDT_Init
	__end_of_WDT_Init:
;; =============== function _WDT_Init ends ============

	signat	_WDT_Init,88
	global	_CLR_BANK1_RAM
psect	text80,local,class=CODE,delta=2
global __ptext80
__ptext80:

;; *************** function _CLR_BANK1_RAM *****************
;; Defined at:
;;		line 150 in file "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
;; Parameters:    Size  Location     Type
;;		None
;; Auto vars:     Size  Location     Type
;;		None
;; Return value:  Size  Location     Type
;;		None               void
;; Registers used:
;;		None
;; Tracked objects:
;;		On entry : 0/0
;;		On exit  : 0/0
;;		Unchanged: FFE00/0
;; Data sizes:     COMMON   BANK0
;;      Params:         0       0
;;      Locals:         0       0
;;      Temps:          0       0
;;      Totals:         0       0
;;Total ram usage:        0 bytes
;; Hardware stack levels used:    1
;; Hardware stack levels required when called:    1
;; This function calls:
;;		Nothing
;; This function is called by:
;;		_main
;; This function uses a non-reentrant model
;;
psect	text80
	file	"E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
	line	150
	global	__size_of_CLR_BANK1_RAM
	__size_of_CLR_BANK1_RAM	equ	__end_of_CLR_BANK1_RAM-_CLR_BANK1_RAM
	
_CLR_BANK1_RAM:	
	opt	stack 6
; Regs used in _CLR_BANK1_RAM: []
	line	152
	
l1270:	
# 152 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVLW (0x80 | 03FH) ;#
	line	153
# 153 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVWF _FSR ;#
	line	154
# 154 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVLW 020H ;#
	line	155
# 155 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVWF 020H ;#
	line	157
# 157 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 BANK1_RAM_CLR_LOOP: ;#
	line	158
# 158 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 CLRF _INDF ;#
	line	159
# 159 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 DECF _FSR,F ;#
	line	160
# 160 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 DECFSZ 020H,F ;#
	line	161
# 161 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 GOTO BANK1_RAM_CLR_LOOP ;#
	line	162
# 162 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 RETURN ;#
psect	text80
	line	164
	
l863:	
	return
	opt stack 0
GLOBAL	__end_of_CLR_BANK1_RAM
	__end_of_CLR_BANK1_RAM:
;; =============== function _CLR_BANK1_RAM ends ============

	signat	_CLR_BANK1_RAM,88
	global	_CLR_BANK0_RAM
psect	text81,local,class=CODE,delta=2
global __ptext81
__ptext81:

;; *************** function _CLR_BANK0_RAM *****************
;; Defined at:
;;		line 129 in file "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
;; Parameters:    Size  Location     Type
;;		None
;; Auto vars:     Size  Location     Type
;;		None
;; Return value:  Size  Location     Type
;;		None               void
;; Registers used:
;;		None
;; Tracked objects:
;;		On entry : 17F/0
;;		On exit  : 0/0
;;		Unchanged: FFE00/0
;; Data sizes:     COMMON   BANK0
;;      Params:         0       0
;;      Locals:         0       0
;;      Temps:          0       0
;;      Totals:         0       0
;;Total ram usage:        0 bytes
;; Hardware stack levels used:    1
;; Hardware stack levels required when called:    1
;; This function calls:
;;		Nothing
;; This function is called by:
;;		_main
;; This function uses a non-reentrant model
;;
psect	text81
	file	"E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
	line	129
	global	__size_of_CLR_BANK0_RAM
	__size_of_CLR_BANK0_RAM	equ	__end_of_CLR_BANK0_RAM-_CLR_BANK0_RAM
	
_CLR_BANK0_RAM:	
	opt	stack 6
; Regs used in _CLR_BANK0_RAM: []
	line	131
	
l1268:	
# 131 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVLW 0X5F ;#
	line	132
# 132 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVWF 020H ;#
	line	133
# 133 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVLW 0X7F ;#
	line	134
# 134 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 MOVWF _FSR ;#
	line	136
# 136 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 BANK0_RAM_CLR_LOOP: ;#
	line	137
# 137 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 CLRF _INDF ;#
	line	138
# 138 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 DECF _FSR,F ;#
	line	139
# 139 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 DECFSZ 020H,F ;#
	line	140
# 140 "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
 GOTO BANK0_RAM_CLR_LOOP ;#
psect	text81
	line	142
	
l860:	
	return
	opt stack 0
GLOBAL	__end_of_CLR_BANK0_RAM
	__end_of_CLR_BANK0_RAM:
;; =============== function _CLR_BANK0_RAM ends ============

	signat	_CLR_BANK0_RAM,88
	global	_GPIO_Init
psect	text82,local,class=CODE,delta=2
global __ptext82
__ptext82:

;; *************** function _GPIO_Init *****************
;; Defined at:
;;		line 90 in file "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
;; Parameters:    Size  Location     Type
;;		None
;; Auto vars:     Size  Location     Type
;;		None
;; Return value:  Size  Location     Type
;;		None               void
;; Registers used:
;;		wreg, status,2
;; Tracked objects:
;;		On entry : 17F/0
;;		On exit  : 17F/0
;;		Unchanged: FFE80/0
;; Data sizes:     COMMON   BANK0
;;      Params:         0       0
;;      Locals:         0       0
;;      Temps:          0       0
;;      Totals:         0       0
;;Total ram usage:        0 bytes
;; Hardware stack levels used:    1
;; Hardware stack levels required when called:    1
;; This function calls:
;;		Nothing
;; This function is called by:
;;		_main
;; This function uses a non-reentrant model
;;
psect	text82
	file	"E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
	line	90
	global	__size_of_GPIO_Init
	__size_of_GPIO_Init	equ	__end_of_GPIO_Init-_GPIO_Init
	
_GPIO_Init:	
	opt	stack 6
; Regs used in _GPIO_Init: [wreg+status,2]
	line	91
	
l1242:	
;main.c: 91: OPTION_REG= 0b000000000;
	bsf	status, 5	;RP0=1, select bank1
	clrf	(129)^080h	;volatile
	line	99
	
l1244:	
;main.c: 99: PCON = 0b00100000;
	movlw	(020h)
	movwf	(142)^080h	;volatile
	line	105
	
l1246:	
;main.c: 105: PORTA = 0b00000000;
	bcf	status, 5	;RP0=0, select bank0
	clrf	(5)	;volatile
	line	106
	
l1248:	
;main.c: 106: TRISA = 0b00000000;
	bsf	status, 5	;RP0=1, select bank1
	clrf	(133)^080h	;volatile
	line	107
	
l1250:	
;main.c: 107: PAHCON= 0b11111111;
	movlw	(0FFh)
	movwf	(146)^080h	;volatile
	line	108
	
l1252:	
;main.c: 108: PADCON= 0b11111111;
	movlw	(0FFh)
	movwf	(147)^080h	;volatile
	line	109
	
l1254:	
;main.c: 109: PAIC0 = 0b00000000;
	clrf	(144)^080h	;volatile
	line	111
;main.c: 111: PDCON = 0b11111111;
	movlw	(0FFh)
	bcf	status, 5	;RP0=0, select bank0
	movwf	(14)	;volatile
	line	112
;main.c: 112: PDCON2= 0b11111111;
	movlw	(0FFh)
	bsf	status, 5	;RP0=1, select bank1
	movwf	(147)^080h	;volatile
	line	114
	
l1256:	
;main.c: 114: PORTB = 0b00000000;
	bcf	status, 5	;RP0=0, select bank0
	clrf	(6)	;volatile
	line	115
	
l1258:	
;main.c: 115: TRISB = 0b00000000;
	bsf	status, 5	;RP0=1, select bank1
	clrf	(134)^080h	;volatile
	line	116
	
l1260:	
;main.c: 116: PBIC0 = 0b00000000;
	clrf	(145)^080h	;volatile
	line	117
	
l1262:	
;main.c: 117: WUCON = 0b00000000;
	clrf	(143)^080h	;volatile
	line	118
	
l1264:	
;main.c: 118: ODCON = 0b00000000;
	bcf	status, 5	;RP0=0, select bank0
	clrf	(15)	;volatile
	line	119
	
l1266:	
;main.c: 119: PHCON = 0b11111111;
	movlw	(0FFh)
	movwf	(16)	;volatile
	line	121
	
l857:	
	return
	opt stack 0
GLOBAL	__end_of_GPIO_Init
	__end_of_GPIO_Init:
;; =============== function _GPIO_Init ends ============

	signat	_GPIO_Init,88
	global	_myIsr
psect	text83,local,class=CODE,delta=2
global __ptext83
__ptext83:

;; *************** function _myIsr *****************
;; Defined at:
;;		line 19 in file "E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
;; Parameters:    Size  Location     Type
;;		None
;; Auto vars:     Size  Location     Type
;;		None
;; Return value:  Size  Location     Type
;;		None               void
;; Registers used:
;;		None
;; Tracked objects:
;;		On entry : 0/0
;;		On exit  : 60/0
;;		Unchanged: FFF9F/0
;; Data sizes:     COMMON   BANK0
;;      Params:         0       0
;;      Locals:         0       0
;;      Temps:          2       0
;;      Totals:         2       0
;;Total ram usage:        2 bytes
;; Hardware stack levels used:    1
;; This function calls:
;;		Nothing
;; This function is called by:
;;		Interrupt level 1
;; This function uses a non-reentrant model
;;
psect	text83
	file	"E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_WDT\main.c"
	line	19
	global	__size_of_myIsr
	__size_of_myIsr	equ	__end_of_myIsr-_myIsr
	
_myIsr:	
	opt	stack 6
; Regs used in _myIsr: []
psect	intentry,class=CODE,delta=2
global __pintentry
__pintentry:
global interrupt_function
interrupt_function:
	global saved_w
	saved_w	set	btemp+0
	movwf	saved_w
	swapf	status,w
	movwf	(??_myIsr+0)
	movf	pclath,w
	movwf	(??_myIsr+1)
	ljmp	_myIsr
psect	text83
	line	20
	
i1l1238:	
;main.c: 20: if(FT0IF)
	bcf	status, 5	;RP0=0, select bank0
	bcf	status, 6	;RP1=0, select bank0
	btfss	(96/8),(96)&7
	goto	u1_21
	goto	u1_20
u1_21:
	goto	i1l842
u1_20:
	line	22
	
i1l1240:	
;main.c: 21: {
;main.c: 22: FT0IF = 0;
	bcf	(96/8),(96)&7
	line	23
;main.c: 23: PORTB = PORTB^0xff;
	comf	(6),f	;volatile
	line	25
	
i1l842:	
	movf	(??_myIsr+1),w
	movwf	pclath
	swapf	(??_myIsr+0)^0FFFFFF80h,w
	movwf	status
	swapf	saved_w,f
	swapf	saved_w,w
	retfie
	opt stack 0
GLOBAL	__end_of_myIsr
	__end_of_myIsr:
;; =============== function _myIsr ends ============

	signat	_myIsr,88
psect	text84,local,class=CODE,delta=2
global __ptext84
__ptext84:
	global	btemp
	btemp set 07Eh

	DABS	1,126,2	;btemp
	global	wtemp0
	wtemp0 set btemp
	end
