__S0 95 0 ABS
__S1 72 0 ABS
_FSR 4 0 ABS
__Hintentry A 0 CODE
__Lintentry 4 0 CODE
__pintentry 4 0 CODE
_TC0H 14 0 ABS
_TC0L 11 0 ABS
_TC0M 12 0 ABS
_FGIE 5F 0 ABS
_INDF 0 0 ABS
_OSCM 94 0 ABS
_PCON 8E 0 ABS
_main 76 0 CODE
btemp 7E 0 ABS
_exit A 0 CODE
start A 0 CODE
_PAIC0 90 0 ABS
_PBIC0 91 0 ABS
_FT0IF 60 0 ABS
_FPBIF 61 0 ABS
_TRISA 85 0 ABS
_TRISB 86 0 ABS
_PORTA 5 0 ABS
reset_vec 0 0 CODE
_FWDTE 477 0 ABS
_PORTB 6 0 ABS
_ODCON F 0 ABS
_PDCON E 0 ABS
_PHCON 10 0 ABS
_WUCON 8F 0 ABS
wtemp0 7E 0 ABS
interrupt_function 4 0 CODE
__Hconfig 0 0 CONFIG
__Lconfig 0 0 CONFIG
__Hram 0 0 ABS
__Lram 0 0 ABS
?_main 70 0 COMMON
_myIsr 35 0 CODE
__Hfunctab 0 0 CODE
__Lfunctab 0 0 CODE
_PDCON2 93 0 ABS
_OPTION_REG 81 0 ABS
__Hcommon 0 0 ABS
__Lcommon 0 0 ABS
__Heeprom_data 0 0 EEDATA
__Leeprom_data 0 0 EEDATA
_FTC0IE 5B 0 ABS
_FTC0IF 63 0 ABS
_FINTIF 62 0 ABS
_PADCON 93 0 ABS
_PAHCON 92 0 ABS
__Habs1 0 0 ABS
__Labs1 0 0 ABS
_FTC0TR 97 0 ABS
_PWMCON 17 0 ABS
__Hsfr0 0 0 ABS
__Lsfr0 0 0 ABS
__Hsfr1 0 0 ABS
__Lsfr1 0 0 ABS
__Hsfr2 0 0 ABS
__Lsfr2 0 0 ABS
__Hsfr3 0 0 ABS
__Lsfr3 0 0 ABS
?_TC0_SLEEP_SET 70 0 COMMON
__Hcode 0 0 ABS
__Lcode 0 0 ABS
??_main 72 0 COMMON
??_GPIO_Init 72 0 COMMON
?_myIsr 70 0 COMMON
saved_w 7E 0 ABS
__Hinit A 0 CODE
__Linit A 0 CODE
__end_of_main 80 0 CODE
__Htext 0 0 ABS
__Ltext 0 0 ABS
end_of_initialization 93 0 CODE
_GPIO_Init 58 0 CODE
__size_of_TC0_SLEEP_SET 0 0 ABS
__Hstrings 0 0 ABS
__Lstrings 0 0 ABS
__Hbank0 0 0 ABS
__Lbank0 0 0 ABS
__Hbank1 0 0 BANK1
__Lbank1 0 0 BANK1
__Hbank2 0 0 BANK2
__Lbank2 0 0 BANK2
__Hbank3 0 0 BANK3
__Lbank3 0 0 BANK3
__Hpowerup 0 0 CODE
__Lpowerup 0 0 CODE
?_CLR_BANK0_RAM 70 0 COMMON
__Hclrtext 0 0 ABS
__Lclrtext 0 0 ABS
?_CLR_BANK1_RAM 70 0 COMMON
__end_of_myIsr 58 0 CODE
??_TC0_SLEEP_SET 72 0 COMMON
__Hidloc 0 0 IDLOC
__Lidloc 0 0 IDLOC
??_myIsr 70 0 COMMON
__end_of_CLR_BANK0_RAM 93 0 CODE
__end_of_CLR_BANK1_RAM 8A 0 CODE
__Hcinit 0 0 ABS
__Lcinit 0 0 ABS
__size_of_main 0 0 ABS
__end_of_GPIO_Init 76 0 CODE
_TC0_SLEEP_SET B 0 CODE
__end_of_TC0_SLEEP_SET 35 0 CODE
?_GPIO_Init 70 0 COMMON
__ptext70 58 0 CODE
__ptext71 35 0 CODE
_CLR_BANK0_RAM 8A 0 CODE
__ptext72 0 0 CODE
_CLR_BANK1_RAM 80 0 CODE
__ptext66 0 0 CODE
__ptext67 B 0 CODE
__ptext68 80 0 CODE
__ptext69 8A 0 CODE
__Hend_init B 0 CODE
__Lend_init A 0 CODE
__Hreset_vec 1 0 CODE
__Lreset_vec 0 0 CODE
_FCOMINTF 69 0 ABS
intlevel0 0 0 CODE
intlevel1 0 0 CODE
intlevel2 0 0 CODE
intlevel3 0 0 CODE
intlevel4 0 0 CODE
intlevel5 0 0 CODE
__size_of_CLR_BANK0_RAM 0 0 ABS
__size_of_CLR_BANK1_RAM 0 0 ABS
??_CLR_BANK0_RAM 72 0 COMMON
__HcstackCOMMON 0 0 ABS
__LcstackCOMMON 0 0 ABS
__size_of_GPIO_Init 0 0 ABS
__pcstackCOMMON 70 0 COMMON
start_initialization 93 0 CODE
__Hmaintext 0 0 ABS
__Lmaintext 0 0 ABS
__pmaintext 76 0 CODE
??_CLR_BANK1_RAM 72 0 COMMON
__size_of_myIsr 0 0 ABS
%segments
reset_vec 0 1 CODE 0
intentry 8 129 CODE 8
cstackCOMMON 70 71 COMMON 70
%locals
startup.obj
startup.as
66 0 0 CODE
75 A 0 CODE
HS16F1211_SLEEP.obj
HS16F1211_SLEEP.as
127 93 0 CODE
128 94 0 CODE
E:\02-HS-DemoCode-Every\C_Code\HS16F1211_cCode\HS16F1211_SLEEP\main.c
53 76 0 CODE
55 77 0 CODE
56 78 0 CODE
72 79 0 CODE
73 7A 0 CODE
75 7D 0 CODE
84 80 0 CODE
201 B 0 CODE
202 D 0 CODE
204 F 0 CODE
215 10 0 CODE
223 12 0 CODE
224 13 0 CODE
225 16 0 CODE
226 18 0 CODE
227 19 0 CODE
228 1A 0 CODE
230 1B 0 CODE
231 1E 0 CODE
239 20 0 CODE
240 21 0 CODE
241 22 0 CODE
243 23 0 CODE
244 29 0 CODE
246 2A 0 CODE
247 2B 0 CODE
248 2E 0 CODE
249 2F 0 CODE
251 31 0 CODE
252 34 0 CODE
389 80 0 CODE
390 81 0 CODE
391 82 0 CODE
392 83 0 CODE
395 84 0 CODE
396 85 0 CODE
397 86 0 CODE
398 87 0 CODE
399 88 0 CODE
401 89 0 CODE
368 8A 0 CODE
369 8B 0 CODE
370 8C 0 CODE
371 8D 0 CODE
374 8E 0 CODE
375 8F 0 CODE
376 90 0 CODE
377 91 0 CODE
379 92 0 CODE
328 58 0 CODE
336 5A 0 CODE
342 5C 0 CODE
343 5E 0 CODE
344 60 0 CODE
345 62 0 CODE
346 64 0 CODE
348 65 0 CODE
349 68 0 CODE
351 6B 0 CODE
352 6D 0 CODE
353 6F 0 CODE
354 70 0 CODE
355 71 0 CODE
356 73 0 CODE
358 75 0 CODE
22 35 0 CODE
24 3B 0 CODE
27 3C 0 CODE
29 40 0 CODE
30 41 0 CODE
32 42 0 CODE
34 46 0 CODE
37 47 0 CODE
39 4B 0 CODE
42 4C 0 CODE
44 50 0 CODE
47 51 0 CODE
21 4 0 CODE
